#

##

##

    礦ision Build Log
    Project:
    F:\佳显电子\新程序\GUI程序制作\GDEW0154T8_UC8151C-20200508\USER\EPD.uvproj
    Project File Date:  03/24/2020

    Output:
    Build target 'Target 1'
    compiling main.c...
    linking...
    Program Size: Code=9124 RO-data=24580 RW-data=92 ZI-data=4748
    FromELF: creating hex file...
    "..\OBJ\EPD.axf" - 0 Error(s), 0 Warning(s).
    Load "..\\OBJ\\EPD.axf"
    Set JLink Project File to "F:\佳显电子\新程序\GUI程序制作\GDEW0154T8_UC8151C-20200508\USER\JLinkSettings.ini"
    * JLink Info: Device "STM32F103VE" selected (512 KB flash, 64 KB RAM).

    JLink info:
    ------------
    DLL: V4.76d, compiled Sep 13 2013 16:35:06
    Firmware: J-Link ARM-OB STM32 compiled Aug 22 2012 19:52:04
    Hardware: V7.00
    S/N : 20090928
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFull

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103VE
    VTarget = 3.300V
    State of Pins:
    TCK: 0, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 4000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...

ng ... are: V7.00 S/N : 20090928 Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFull * JLink Info: Found SWD-DP with ID 0x1BA01477 * JLink Info: Found SWD-DP with ID 0x1BA01477 * JLink Info: Found Cortex-M3 r1p1, Little endian. * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots * JLink Info: TPIU fitted. * JLink Info: ETM fitted. ROMTableAddr = 0xE00FF003 Target info: ------------ Device: STM32F103VE VTarget = 3.300V State of Pins: TCK: 0, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1 Hardware-Breakpoints: 6 Software-Breakpoints: 8192 Watchpoints: 4 JTAG speed: 4000 kHz No Algorithm found for: 08000000H - 080083CFH Erase skipped! Error: Flash Download failed - "Cortex-M3" Load "..\\OBJ\\OLED.axf" Set JLink Project File to "F:\佳显电子\新程序\GUI程序制作\GDEW0154T8_UC8151C-20200508\USER\JLinkSettings.ini" * JLink Info: Device "STM32F103VE" selected (512 KB flash, 64 KB RAM). JLink info: ------------ DLL: V4.76d, compiled Sep 13 2013 16:35:06 Firmware: J-Link ARM-OB STM32 compiled Aug 22 2012 19:52:04 Hardware: V7.00 S/N : 20090928 Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFull * JLink Info: Found SWD-DP with ID 0x1BA01477 * JLink Info: Found SWD-DP with ID 0x1BA01477 * JLink Info: Found Cortex-M3 r1p1, Little endian. * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots * JLink Info: TPIU fitted. * JLink Info: ETM fitted. ROMTableAddr = 0xE00FF003 Target info: ------------ Device: STM32F103VE VTarget = 3.300V State of Pins: TCK: 0, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1 Hardware-Breakpoints: 6 Software-Breakpoints: 8192 Watchpoints: 4 JTAG speed: 4000 kHz Erase Done. Programming Done. Verify OK. Application running ...