state.Zero {
	control.1 {
		iface MIXER
		name 'Mic 1 Volume'
		value 0
		comment {
			access 'read write'
			type INTEGER
			count 1
			range '0 - 7'
			dbmin -600
			dbmax 3600
			dbvalue.0 -600
		}
	}
	control.2 {
		iface MIXER
		name 'Mic 2 Volume'
		value 6
		comment {
			access 'read write'
			type INTEGER
			count 1
			range '0 - 7'
			dbmin -600
			dbmax 3600
			dbvalue.0 3000
		}
	}
	control.3 {
		iface MIXER
		name 'Aux Volume'
		value.0 0
		value.1 0
		comment {
			access 'read write'
			type INTEGER
			count 2
			range '0 - 63'
			dbmin -5400
			dbmax 1500
			dbvalue.0 -5400
			dbvalue.1 -5400
		}
	}
	control.4 {
		iface MIXER
		name 'Mixin PGA Volume'
		value.0 0
		value.1 0
		comment {
			access 'read write'
			type INTEGER
			count 2
			range '0 - 15'
			dbmin -450
			dbmax 1800
			dbvalue.0 -450
			dbvalue.1 -450
		}
	}
	control.5 {
		iface MIXER
		name 'ADC Volume'
		value.0 114
		value.1 114
		comment {
			access 'read write'
			type INTEGER
			count 2
			range '0 - 127'
			dbmin -9999999
			dbmax 1125
			dbvalue.0 150
			dbvalue.1 150
		}
	}
	control.6 {
		iface MIXER
		name 'DAC Volume'
		value.0 7
		value.1 7
		comment {
			access 'read write'
			type INTEGER
			count 2
			range '0 - 127'
			dbmin -9999999
			dbmax 1125
			dbvalue.0 -9999999
			dbvalue.1 -9999999
		}
	}
	control.7 {
		iface MIXER
		name 'Headphone Volume'
		value.0 0
		value.1 0
		comment {
			access 'read write'
			type INTEGER
			count 2
			range '0 - 63'
			dbmin -5700
			dbmax 600
			dbvalue.0 -5700
			dbvalue.1 -5700
		}
	}
	control.8 {
		iface MIXER
		name 'Lineout Volume'
		value 0
		comment {
			access 'read write'
			type INTEGER
			count 1
			range '0 - 63'
			dbmin -4800
			dbmax 1500
			dbvalue.0 -4800
		}
	}
	control.9 {
		iface MIXER
		name 'DAC EQ Switch'
		value false
		comment {
			access 'read write'
			type BOOLEAN
			count 1
		}
	}
	control.10 {
		iface MIXER
		name 'DAC EQ1 Volume'
		value 0
		comment {
			access 'read write'
			type INTEGER
			count 1
			range '0 - 15'
			dbmin -1050
			dbmax 1200
			dbvalue.0 -1050
		}
	}
	control.11 {
		iface MIXER
		name 'DAC EQ2 Volume'
		value 0
		comment {
			access 'read write'
			type INTEGER
			count 1
			range '0 - 15'
			dbmin -1050
			dbmax 1200
			dbvalue.0 -1050
		}
	}
	control.12 {
		iface MIXER
		name 'DAC EQ3 Volume'
		value 0
		comment {
			access 'read write'
			type INTEGER
			count 1
			range '0 - 15'
			dbmin -1050
			dbmax 1200
			dbvalue.0 -1050
		}
	}
	control.13 {
		iface MIXER
		name 'DAC EQ4 Volume'
		value 0
		comment {
			access 'read write'
			type INTEGER
			count 1
			range '0 - 15'
			dbmin -1050
			dbmax 1200
			dbvalue.0 -1050
		}
	}
	control.14 {
		iface MIXER
		name 'DAC EQ5 Volume'
		value 0
		comment {
			access 'read write'
			type INTEGER
			count 1
			range '0 - 15'
			dbmin -1050
			dbmax 1200
			dbvalue.0 -1050
		}
	}
	control.15 {
		iface MIXER
		name 'ADC HPF Switch'
		value false
		comment {
			access 'read write'
			type BOOLEAN
			count 1
		}
	}
	control.16 {
		iface MIXER
		name 'ADC HPF Cutoff'
		value Fs/24000
		comment {
			access 'read write'
			type ENUMERATED
			count 1
			item.0 Fs/24000
			item.1 Fs/12000
			item.2 Fs/6000
			item.3 Fs/3000
		}
	}
	control.17 {
		iface MIXER
		name 'ADC Voice Mode Switch'
		value false
		comment {
			access 'read write'
			type BOOLEAN
			count 1
		}
	}
	control.18 {
		iface MIXER
		name 'ADC Voice Cutoff'
		value '2.5Hz'
		comment {
			access 'read write'
			type ENUMERATED
			count 1
			item.0 '2.5Hz'
			item.1 '25Hz'
			item.2 '50Hz'
			item.3 '100Hz'
			item.4 '150Hz'
			item.5 '200Hz'
			item.6 '300Hz'
			item.7 '400Hz'
		}
	}
	control.19 {
		iface MIXER
		name 'DAC HPF Switch'
		value false
		comment {
			access 'read write'
			type BOOLEAN
			count 1
		}
	}
	control.20 {
		iface MIXER
		name 'DAC HPF Cutoff'
		value Fs/24000
		comment {
			access 'read write'
			type ENUMERATED
			count 1
			item.0 Fs/24000
			item.1 Fs/12000
			item.2 Fs/6000
			item.3 Fs/3000
		}
	}
	control.21 {
		iface MIXER
		name 'DAC Voice Mode Switch'
		value false
		comment {
			access 'read write'
			type BOOLEAN
			count 1
		}
	}
	control.22 {
		iface MIXER
		name 'DAC Voice Cutoff'
		value '2.5Hz'
		comment {
			access 'read write'
			type ENUMERATED
			count 1
			item.0 '2.5Hz'
			item.1 '25Hz'
			item.2 '50Hz'
			item.3 '100Hz'
			item.4 '150Hz'
			item.5 '200Hz'
			item.6 '300Hz'
			item.7 '400Hz'
		}
	}
	control.23 {
		iface MIXER
		name 'Mic 1 Switch'
		value false
		comment {
			access 'read write'
			type BOOLEAN
			count 1
		}
	}
	control.24 {
		iface MIXER
		name 'Mic 2 Switch'
		value true
		comment {
			access 'read write'
			type BOOLEAN
			count 1
		}
	}
	control.25 {
		iface MIXER
		name 'Aux Switch'
		value.0 false
		value.1 false
		comment {
			access 'read write'
			type BOOLEAN
			count 2
		}
	}
	control.26 {
		iface MIXER
		name 'Mixin PGA Switch'
		value.0 true
		value.1 true
		comment {
			access 'read write'
			type BOOLEAN
			count 2
		}
	}
	control.27 {
		iface MIXER
		name 'ADC Switch'
		value.0 true
		value.1 true
		comment {
			access 'read write'
			type BOOLEAN
			count 2
		}
	}
	control.28 {
		iface MIXER
		name 'Headphone Switch'
		value.0 false
		value.1 false
		comment {
			access 'read write'
			type BOOLEAN
			count 2
		}
	}
	control.29 {
		iface MIXER
		name 'Lineout Switch'
		value false
		comment {
			access 'read write'
			type BOOLEAN
			count 1
		}
	}
	control.30 {
		iface MIXER
		name 'DAC Soft Mute Switch'
		value false
		comment {
			access 'read write'
			type BOOLEAN
			count 1
		}
	}
	control.31 {
		iface MIXER
		name 'DAC Soft Mute Rate'
		value '1'
		comment {
			access 'read write'
			type ENUMERATED
			count 1
			item.0 '1'
			item.1 '2'
			item.2 '4'
			item.3 '8'
			item.4 '16'
			item.5 '32'
			item.6 '64'
		}
	}
	control.32 {
		iface MIXER
		name 'Aux ZC Switch'
		value.0 false
		value.1 false
		comment {
			access 'read write'
			type BOOLEAN
			count 2
		}
	}
	control.33 {
		iface MIXER
		name 'Mixin PGA ZC Switch'
		value.0 true
		value.1 true
		comment {
			access 'read write'
			type BOOLEAN
			count 2
		}
	}
	control.34 {
		iface MIXER
		name 'Headphone ZC Switch'
		value.0 false
		value.1 false
		comment {
			access 'read write'
			type BOOLEAN
			count 2
		}
	}
	control.35 {
		iface MIXER
		name 'ToneGen Volume'
		value 0
		comment {
			access 'read write'
			type INTEGER
			count 1
			range '0 - 15'
			dbmin -4500
			dbmax 0
			dbvalue.0 -4500
		}
	}
	control.36 {
		iface MIXER
		name 'ToneGen DTMF Key'
		value '0'
		comment {
			access 'read write'
			type ENUMERATED
			count 1
			item.0 '0'
			item.1 '1'
			item.2 '2'
			item.3 '3'
			item.4 '4'
			item.5 '5'
			item.6 '6'
			item.7 '7'
			item.8 '8'
			item.9 '9'
			item.10 A
			item.11 B
			item.12 C
			item.13 D
			item.14 '*'
			item.15 '#'
		}
	}
	control.37 {
		iface MIXER
		name 'ToneGen DTMF Switch'
		value false
		comment {
			access 'read write'
			type BOOLEAN
			count 1
		}
	}
	control.38 {
		iface MIXER
		name 'ToneGen Start'
		value false
		comment {
			access 'read write'
			type BOOLEAN
			count 1
		}
	}
	control.39 {
		iface MIXER
		name 'ToneGen Sinewave Gen Type'
		value Sum
		comment {
			access 'read write'
			type ENUMERATED
			count 1
			item.0 Sum
			item.1 SWG1
			item.2 SWG2
			item.3 Sum
		}
	}
	control.40 {
		iface MIXER
		name 'ToneGen Sinewave1 Freq'
		value 0
		comment {
			access 'read write'
			type INTEGER
			count 1
			range '0 - 65535'
		}
	}
	control.41 {
		iface MIXER
		name 'ToneGen Sinewave2 Freq'
		value 0
		comment {
			access 'read write'
			type INTEGER
			count 1
			range '0 - 65535'
		}
	}
	control.42 {
		iface MIXER
		name 'ToneGen On Time'
		value 0
		comment {
			access 'read write'
			type INTEGER
			count 1
			range '0 - 63'
		}
	}
	control.43 {
		iface MIXER
		name 'ToneGen Off Time'
		value 0
		comment {
			access 'read write'
			type INTEGER
			count 1
			range '0 - 63'
		}
	}
	control.44 {
		iface MIXER
		name 'Aux Gain Ramping Switch'
		value.0 false
		value.1 false
		comment {
			access 'read write'
			type BOOLEAN
			count 2
		}
	}
	control.45 {
		iface MIXER
		name 'Mixin Gain Ramping Switch'
		value.0 false
		value.1 false
		comment {
			access 'read write'
			type BOOLEAN
			count 2
		}
	}
	control.46 {
		iface MIXER
		name 'ADC Gain Ramping Switch'
		value.0 false
		value.1 false
		comment {
			access 'read write'
			type BOOLEAN
			count 2
		}
	}
	control.47 {
		iface MIXER
		name 'DAC Gain Ramping Switch'
		value.0 false
		value.1 false
		comment {
			access 'read write'
			type BOOLEAN
			count 2
		}
	}
	control.48 {
		iface MIXER
		name 'Headphone Gain Ramping Switch'
		value.0 false
		value.1 false
		comment {
			access 'read write'
			type BOOLEAN
			count 2
		}
	}
	control.49 {
		iface MIXER
		name 'Lineout Gain Ramping Switch'
		value false
		comment {
			access 'read write'
			type BOOLEAN
			count 1
		}
	}
	control.50 {
		iface MIXER
		name 'Gain Ramping Rate'
		value 'nominal rate * 8'
		comment {
			access 'read write'
			type ENUMERATED
			count 1
			item.0 'nominal rate * 8'
			item.1 'nominal rate * 16'
			item.2 'nominal rate / 16'
			item.3 'nominal rate / 32'
		}
	}
	control.51 {
		iface MIXER
		name 'DAC NG Switch'
		value false
		comment {
			access 'read write'
			type BOOLEAN
			count 1
		}
	}
	control.52 {
		iface MIXER
		name 'DAC NG Setup Time'
		value '256 samples'
		comment {
			access 'read write'
			type ENUMERATED
			count 1
			item.0 '256 samples'
			item.1 '512 samples'
			item.2 '1024 samples'
			item.3 '2048 samples'
		}
	}
	control.53 {
		iface MIXER
		name 'DAC NG Rampup Rate'
		value '0.02 ms/dB'
		comment {
			access 'read write'
			type ENUMERATED
			count 1
			item.0 '0.02 ms/dB'
			item.1 '0.16 ms/dB'
		}
	}
	control.54 {
		iface MIXER
		name 'DAC NG Rampdown Rate'
		value '0.64 ms/dB'
		comment {
			access 'read write'
			type ENUMERATED
			count 1
			item.0 '0.64 ms/dB'
			item.1 '20.48 ms/dB'
		}
	}
	control.55 {
		iface MIXER
		name 'DAC NG OFF Threshold'
		value 0
		comment {
			access 'read write'
			type INTEGER
			count 1
			range '0 - 7'
		}
	}
	control.56 {
		iface MIXER
		name 'DAC NG ON Threshold'
		value 0
		comment {
			access 'read write'
			type INTEGER
			count 1
			range '0 - 7'
		}
	}
	control.57 {
		iface MIXER
		name 'DAC Mono Switch'
		value.0 false
		value.1 false
		comment {
			access 'read write'
			type BOOLEAN
			count 2
		}
	}
	control.58 {
		iface MIXER
		name 'DAC Invert Switch'
		value.0 false
		value.1 false
		comment {
			access 'read write'
			type BOOLEAN
			count 2
		}
	}
	control.59 {
		iface MIXER
		name 'DMIC Switch'
		value.0 false
		value.1 false
		comment {
			access 'read write'
			type BOOLEAN
			count 2
		}
	}
	control.60 {
		iface MIXER
		name 'ALC Switch'
		value.0 false
		value.1 false
		comment {
			access 'read write'
			type BOOLEAN
			count 2
		}
	}
	control.61 {
		iface MIXER
		name 'ALC Attack Rate'
		value '44/fs'
		comment {
			access 'read write'
			type ENUMERATED
			count 1
			item.0 '44/fs'
			item.1 '88/fs'
			item.2 '176/fs'
			item.3 '352/fs'
			item.4 '704/fs'
			item.5 '1408/fs'
			item.6 '2816/fs'
			item.7 '5632/fs'
			item.8 '11264/fs'
			item.9 '22528/fs'
			item.10 '45056/fs'
			item.11 '90112/fs'
			item.12 '180224/fs'
		}
	}
	control.62 {
		iface MIXER
		name 'ALC Release Rate'
		value '176/fs'
		comment {
			access 'read write'
			type ENUMERATED
			count 1
			item.0 '176/fs'
			item.1 '352/fs'
			item.2 '704/fs'
			item.3 '1408/fs'
			item.4 '2816/fs'
			item.5 '5632/fs'
			item.6 '11264/fs'
			item.7 '22528/fs'
			item.8 '45056/fs'
			item.9 '90112/fs'
			item.10 '180224/fs'
		}
	}
	control.63 {
		iface MIXER
		name 'ALC Hold Time'
		value '62/fs'
		comment {
			access 'read write'
			type ENUMERATED
			count 1
			item.0 '62/fs'
			item.1 '124/fs'
			item.2 '248/fs'
			item.3 '496/fs'
			item.4 '992/fs'
			item.5 '1984/fs'
			item.6 '3968/fs'
			item.7 '7936/fs'
			item.8 '15872/fs'
			item.9 '31744/fs'
			item.10 '63488/fs'
			item.11 '126976/fs'
			item.12 '253952/fs'
			item.13 '507904/fs'
			item.14 '1015808/fs'
			item.15 '2031616/fs'
		}
	}
	control.64 {
		iface MIXER
		name 'ALC Integ Attack Rate'
		value '1/4'
		comment {
			access 'read write'
			type ENUMERATED
			count 1
			item.0 '1/4'
			item.1 '1/16'
			item.2 '1/256'
			item.3 '1/65536'
		}
	}
	control.65 {
		iface MIXER
		name 'ALC Integ Release Rate'
		value '1/4'
		comment {
			access 'read write'
			type ENUMERATED
			count 1
			item.0 '1/4'
			item.1 '1/16'
			item.2 '1/256'
			item.3 '1/65536'
		}
	}
	control.66 {
		iface MIXER
		name 'ALC Noise Threshold Volume'
		value 0
		comment {
			access 'read write'
			type INTEGER
			count 1
			range '0 - 63'
			dbmin -9450
			dbmax 0
			dbvalue.0 -9450
		}
	}
	control.67 {
		iface MIXER
		name 'ALC Min Threshold Volume'
		value 0
		comment {
			access 'read write'
			type INTEGER
			count 1
			range '0 - 63'
			dbmin -9450
			dbmax 0
			dbvalue.0 -9450
		}
	}
	control.68 {
		iface MIXER
		name 'ALC Max Threshold Volume'
		value 0
		comment {
			access 'read write'
			type INTEGER
			count 1
			range '0 - 63'
			dbmin -9450
			dbmax 0
			dbvalue.0 -9450
		}
	}
	control.69 {
		iface MIXER
		name 'ALC Max Attenuation Volume'
		value 0
		comment {
			access 'read write'
			type INTEGER
			count 1
			range '0 - 15'
			dbmin 0
			dbmax 9000
			dbvalue.0 0
		}
	}
	control.70 {
		iface MIXER
		name 'ALC Max Gain Volume'
		value 0
		comment {
			access 'read write'
			type INTEGER
			count 1
			range '0 - 15'
			dbmin 0
			dbmax 9000
			dbvalue.0 0
		}
	}
	control.71 {
		iface MIXER
		name 'ALC Min Analog Gain Volume'
		value 0
		comment {
			access 'read write'
			type INTEGER
			count 1
			range '0 - 7'
			dbmin -9999999
			dbmax 3600
			dbvalue.0 -9999999
		}
	}
	control.72 {
		iface MIXER
		name 'ALC Max Analog Gain Volume'
		value 0
		comment {
			access 'read write'
			type INTEGER
			count 1
			range '0 - 7'
			dbmin -9999999
			dbmax 3600
			dbvalue.0 -9999999
		}
	}
	control.73 {
		iface MIXER
		name 'ALC Anticlip Mode Switch'
		value false
		comment {
			access 'read write'
			type BOOLEAN
			count 1
		}
	}
	control.74 {
		iface MIXER
		name 'ALC Anticlip Level'
		value 0
		comment {
			access 'read write'
			type INTEGER
			count 1
			range '0 - 127'
		}
	}
	control.75 {
		iface MIXER
		name 'HP Jack Switch'
		value false
		comment {
			access 'read write'
			type BOOLEAN
			count 1
		}
	}
	control.76 {
		iface MIXER
		name 'MIC Jack Switch'
		value false
		comment {
			access 'read write'
			type BOOLEAN
			count 1
		}
	}
	control.77 {
		iface MIXER
		name 'Onboard MIC Switch'
		value true
		comment {
			access 'read write'
			type BOOLEAN
			count 1
		}
	}
	control.78 {
		iface MIXER
		name 'AUX Jack Switch'
		value false
		comment {
			access 'read write'
			type BOOLEAN
			count 1
		}
	}
	control.79 {
		iface MIXER
		name 'Mic 1 Amp Source MUX'
		value Differential
		comment {
			access 'read write'
			type ENUMERATED
			count 1
			item.0 Differential
			item.1 MIC_P
			item.2 MIC_N
		}
	}
	control.80 {
		iface MIXER
		name 'Mic 2 Amp Source MUX'
		value MIC_N
		comment {
			access 'read write'
			type ENUMERATED
			count 1
			item.0 Differential
			item.1 MIC_P
			item.2 MIC_N
		}
	}
	control.81 {
		iface MIXER
		name 'Mixin Left Aux Left Switch'
		value false
		comment {
			access 'read write'
			type BOOLEAN
			count 1
		}
	}
	control.82 {
		iface MIXER
		name 'Mixin Left Mic 1 Switch'
		value false
		comment {
			access 'read write'
			type BOOLEAN
			count 1
		}
	}
	control.83 {
		iface MIXER
		name 'Mixin Left Mic 2 Switch'
		value false
		comment {
			access 'read write'
			type BOOLEAN
			count 1
		}
	}
	control.84 {
		iface MIXER
		name 'Mixin Left Mixin Right Switch'
		value false
		comment {
			access 'read write'
			type BOOLEAN
			count 1
		}
	}
	control.85 {
		iface MIXER
		name 'Mixin Right Aux Right Switch'
		value false
		comment {
			access 'read write'
			type BOOLEAN
			count 1
		}
	}
	control.86 {
		iface MIXER
		name 'Mixin Right Mic 2 Switch'
		value true
		comment {
			access 'read write'
			type BOOLEAN
			count 1
		}
	}
	control.87 {
		iface MIXER
		name 'Mixin Right Mic 1 Switch'
		value false
		comment {
			access 'read write'
			type BOOLEAN
			count 1
		}
	}
	control.88 {
		iface MIXER
		name 'Mixin Right Mixin Left Switch'
		value false
		comment {
			access 'read write'
			type BOOLEAN
			count 1
		}
	}
	control.89 {
		iface MIXER
		name 'DAI Left Source MUX'
		value 'ADC Left'
		comment {
			access 'read write'
			type ENUMERATED
			count 1
			item.0 'ADC Left'
			item.1 'ADC Right'
			item.2 'DAI Input Left'
			item.3 'DAI Input Right'
		}
	}
	control.90 {
		iface MIXER
		name 'DAI Right Source MUX'
		value 'ADC Right'
		comment {
			access 'read write'
			type ENUMERATED
			count 1
			item.0 'ADC Left'
			item.1 'ADC Right'
			item.2 'DAI Input Left'
			item.3 'DAI Input Right'
		}
	}
	control.91 {
		iface MIXER
		name 'DAC Left Source MUX'
		value 'DAI Input Left'
		comment {
			access 'read write'
			type ENUMERATED
			count 1
			item.0 'ADC Output Left'
			item.1 'ADC Output Right'
			item.2 'DAI Input Left'
			item.3 'DAI Input Right'
		}
	}
	control.92 {
		iface MIXER
		name 'DAC Right Source MUX'
		value 'DAI Input Right'
		comment {
			access 'read write'
			type ENUMERATED
			count 1
			item.0 'ADC Output Left'
			item.1 'ADC Output Right'
			item.2 'DAI Input Left'
			item.3 'DAI Input Right'
		}
	}
	control.93 {
		iface MIXER
		name 'Mixout Left Aux Left Switch'
		value false
		comment {
			access 'read write'
			type BOOLEAN
			count 1
		}
	}
	control.94 {
		iface MIXER
		name 'Mixout Left Mixin Left Switch'
		value false
		comment {
			access 'read write'
			type BOOLEAN
			count 1
		}
	}
	control.95 {
		iface MIXER
		name 'Mixout Left Mixin Right Switch'
		value false
		comment {
			access 'read write'
			type BOOLEAN
			count 1
		}
	}
	control.96 {
		iface MIXER
		name 'Mixout Left DAC Left Switch'
		value false
		comment {
			access 'read write'
			type BOOLEAN
			count 1
		}
	}
	control.97 {
		iface MIXER
		name 'Mixout Left Aux Left Invert Switch'
		value false
		comment {
			access 'read write'
			type BOOLEAN
			count 1
		}
	}
	control.98 {
		iface MIXER
		name 'Mixout Left Mixin Left Invert Switch'
		value false
		comment {
			access 'read write'
			type BOOLEAN
			count 1
		}
	}
	control.99 {
		iface MIXER
		name 'Mixout Left Mixin Right Invert Switch'
		value false
		comment {
			access 'read write'
			type BOOLEAN
			count 1
		}
	}
	control.100 {
		iface MIXER
		name 'Mixout Right Aux Right Switch'
		value false
		comment {
			access 'read write'
			type BOOLEAN
			count 1
		}
	}
	control.101 {
		iface MIXER
		name 'Mixout Right Mixin Right Switch'
		value false
		comment {
			access 'read write'
			type BOOLEAN
			count 1
		}
	}
	control.102 {
		iface MIXER
		name 'Mixout Right Mixin Left Switch'
		value false
		comment {
			access 'read write'
			type BOOLEAN
			count 1
		}
	}
	control.103 {
		iface MIXER
		name 'Mixout Right DAC Right Switch'
		value false
		comment {
			access 'read write'
			type BOOLEAN
			count 1
		}
	}
	control.104 {
		iface MIXER
		name 'Mixout Right Aux Right Invert Switch'
		value false
		comment {
			access 'read write'
			type BOOLEAN
			count 1
		}
	}
	control.105 {
		iface MIXER
		name 'Mixout Right Mixin Right Invert Switch'
		value false
		comment {
			access 'read write'
			type BOOLEAN
			count 1
		}
	}
	control.106 {
		iface MIXER
		name 'Mixout Right Mixin Left Invert Switch'
		value false
		comment {
			access 'read write'
			type BOOLEAN
			count 1
		}
	}
}
