STM32f103c8t6
Flash 存储空间：64 KB
SRAM（静态随机存取存储器）：20 KB
功能：
1.最大可以显示460*276像素大小的6色图片。（占用约62kb的Flash）
2.可以创建面积≤39000的矩形空白图像（占用约19.5kb的SRAM），在空白图像范围内可以显示字符和简单的几何图形，支持七种色。
3.
请注意:
1.用户创建的图像不得超过19.5kb
2.显示图像的起始坐标（X，Y），必须满足X+Width≤800&&X+ Height≤480。
3.在空白图像中的绘制的字符、几何图形不得超出所定义图像的范围，要考虑到字符串的长度。



STM32f103c8t6
Flash memory: 64 KB
SRAM (Static Random Access Memory): 20 KB
Function:
1. It can display six-color pictures with a maximum size of 460*276 pixels. (Occupies about 62kb of Flash)
2. A rectangular blank image with an area of ≤39,000 can be created (occupying about 19.5kb of SRAM). 
Characters and simple geometric figures can be displayed within the blank image range, and seven colors are supported.
3.
Please note:
1. User-created images must not exceed 19.5kb
2. The starting coordinates (X, Y) of the displayed image must satisfy X+Width≤800&&X+ Height≤480.
3. The characters and geometric figures drawn in the blank image must not exceed the scope of the defined image,
 and the length of the string must be taken into consideration.

