- Device Information

  Device Name:

  Device MAC:

  Firware Version:V1.

- Network Settings

  IP Addressing:

  IP Address:

  Local Port:

  Mode:

  Subnet Mask:

  Gateway:

  Destination IP/DNS:

  Destination Port:

  Web Port:

- Serial Settings

  Baudrate:

  Data Bits:

  Parity:

  Stop Bits:

  Flow Control:

- Multi-Master Settings

  Protocol:

  Response Timeout: 32~8000ms

  Multi-Master:

  Transmit Delay 5~255ms

  NOTE:When the multi master is disabled, the response timeout will always be 0. The timeout must be a multiple of 32.

- Advanced Settings

  Watchdog Reset:

  Watchdog Reset Time: 5~1270 s

  Re-connect Time: 1~255 s

- Modify Web Password

  New Password:

  Confirm Password:

Copyright © Shengui Technology Co., Ltd. 2022